(****** QuickLD compiler *******************************)
(****** Copyright Rockwell Automation Canada, Ltd ******)
(****** ST *********************************************)

(*************** Rung **********************************)
(*Enter the IP address of the SCT-20 To Tare the scale enter a 7 for the command number.
To Zero The scale enter a 8 for the command number.
To Clear Tare enter a 9 for the command number.*)
(*Label :*)(**)
(* FB call: SCT_20_EIP *)
SCT_20_EIP_1(TRUE, ENTERIPADDRESS, ENTERCOMMAND, ENTERSETPOINT, CHANGEOUT1STATE, CHANGEOUT2STATE, CHANGEOUT3STATE) ;

(*************** Code for the end of Rung **************)


(*************** Code for the end of File **************)
__GL __LG0000 ;



(*************** Local Symbols table *******************)

