line,id,display,keyEventName[0],keyEventName[1],keyEventName[2],titleStart,titleEnd,titleAlign,title[128],textStart,textEnd,textAlign,text

//INPUT  Notice: In CR mode, directly from input to output text in ID10.
253,70,0,,,,0,0,0,,16,23,2,,,

// DOT DISPLAY
// TARE
0,0,1,,,,,,1,,1,14,1,KEY IN ITEM No,
0,0,1,,,,,,1,,15,24,2,[No+PLU],

// SEG DISPLAY
0,4,0,,,,,,1,,0,0,1,,
0,0,0,,,,,,1,,1,23,2,KEY IN ITEM No [No+PLU],


