- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< It detected blackout for the applicator (605)

Error content | Applicator CPU was reset.
Detail | Before receiving the acknowledge power ON command, the applicator received a different command.
Solution | Restore power
Action by user |
Action by service representative |
Related part | ① 24 V DC to the power supply (XJ12) of P-1105 [A100]. ② RS485 communication cable between main boards (P-1100, P-1163, P-1000) [A10] and P-1105 [A100].
Remarks |