< Film is remaining (480 亅 0101)

Error content | Film is remaining.
Detail | The film sensor board is knocked over when the film started to be sent. The bit mask shows the knocked over sensor location. Number and location correlation are as follows: 0001: Rear right 0010: Front right 0100: Rear left 1000: Front left (Ex) If remaining film were detected in the rear right and front right, the sub-error would be 0011.
Solution | Press the [RETURN] button after removing film.
Action by user |
Action by service representative |
Related part | <If the error occurs even after the film is removed> 嘆 P-1105 [A200] 嘇 Film presence front right [B209]. 嘊 Film presence front left [B208]. 嘋 Film presence rear left [B210]. 嘍 Film presence rear right [B211].
Remarks |