- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film feeding error for the lower (466)

Error content | Lower film was not supplied.
Detail | Lower film was sent, but the lower film detection board did not fall down. Sub-error meanings are as follows: 0XXX: Shortly before the operation, no film was changed over. 1XXX: Shortly before the operation, film was changed over. XXX indicates the external diameter of roll [mm] when an error detected. (If an error occurs by the film feeding for the first time after the film loading or the power is turned on, external diameter of roll becomes 0).
Solution | Press the [RETURN] button after checking the lower film.
Action by user |
Action by service representative |
Related part |
Remarks | The error will not be displayed by selection [No] in film error machine settings.