- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■Underlabeller Error (01039)

Error content | There is no label to attach. The label may be jammed. Check the label on the under label printer (Printer 4).
Detail | The product has arrived at the under label applicator, but there is no label to attach. -The label is jammed -The label is not connected to the label transport belt due to adhesion of glue to the cutter blade -The label transport conveyor is dirty
Solution | Touch [OK] after checking and removing the under label.
Action by user | Touch [OK] after checking and removing the under label.
Action by service representative | Make sure that the under label is connected to the label transport conveyor.
Related part |
Remarks |