- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

No film on the lower (464)

Error content | Lower film finished.
Detail | The film detection plate did not fall down by the specified amount when the lower film was being fed. Sub-error meanings are as follows: 0XXX: The film switching operation was not performed immediately before. 1XXX: The film switching operation was performed immediately before. XXX is the film roll outer diameter (mm) when an error is detected.(If an error occurs during the first film feed after loading or power-on, the roll outer diameter will become ”0".)
Solution | Check the lower film, then touch [RETURN].
Action by user | Check the film setting.
Action by service representative |
Related part |
Remarks | This error will not occur when the Film Error is set NO in the machine setting. This error will not occur when the Detail Film End Check is set NO in the wrapping machine setting. Occurs only in overseas special specifications.