- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< It failed in taking product in (515)

Error content | Failed to take in the product.
Detail | Failed to transfer the tray during the transfer process using the feed bar. The sub-error has the following meanings: 0001: The product did not pass through the feed bar ON sensor within the specified time (the sensor did not switch to a floodlighted state). 0002: The tray stop sensor was in a light-shielded state when the feed bar was fully pressed. 0003: The tray stop sensor was shielded before the feed bar ON sensor was shielded. 0012: The tray stop sensor was shielded before the tray separation sensor (front) was shielded.
Release method | Open the cover, remove the product, and press the [RETURN] button.
User’s action | Open the cover, remove the product, and press the [RETURN] button.
Service action |
Relevant locations | 1) P-1105[A600] 2) Tray stop sensor [B606] 3) Feed bar ON sensor [B605] 4) Tray separation sensor (front) [B604]
Remarks |