- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Wrapper is not connected (401)

Error content | Wrapper is not connected.
Detail | Communication error before power has been turned ON. Communication phase No. is listed in the sub-error.
Solution | [STOP] button＝> Cancel error [REEXEC] button => Re-check the connection with the wrapper.
Action by user | Perform turn ON/OFF of the power supply.
Action by service representative |
Related part |
Remarks | After pressing the [STOP] button, only pricing can be performed.