- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■ Thermal head for printer 1 up (00716-0001, 00816-0001, 01016-0001, 01911-0001)

Error content | Thermal head for printer 1 up.
Detail | The thermal head was up when printing starts. *This error is displayed in DP mode.
Solution | Touch [OK] button after setting the thermal head.
Action by user | Touch [OK] button after setting the thermal head.
Action by service representative | Check head-up sensor.
Related part |
Remarks | “Printer No.1” changes depending on error No.