- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Centering motor is abnormal (422)

Error content | The centering motor is abnormal.
Detail | The centering motor operation has not been completed normally. The sub-error has the following meaning: 0001: The operation is not completed though the operation protection timer has expired.
Solution | Press the [RETURN] button. Enter “495344” and press [PLU] to exit the error screen, which enables the use as a weighing printer.
User’s action | Press [RETURN] button to release the error.
Service person’s action | Check the following related parts and repair or replace the defective part(s).
Relevant locations | ① P-1105 [A200] ② P-1006 board for tray presser/centering [A202] ③ Centering motor [M205] ④ Centering origin [B205] ⑤ Defect of the wrapper switching power supply DC 24V is not output. ⑥ When the “0422-0001” error is displayed immediately after “0615-0021” is displayed F104 or F105 fuse (250[V]6[A]) has blown.
Remarks |