- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

<Tray is placed in front (3018)

Error content | Tray is placed in front
Detail | This error occurs when the tray front detection sensor is light-shielded while PS-AI is linked.
Solution | Press the [OK] button.
Action by user | Confirm that the tray front detection sensor is not light-shielded, and then press the [OK] button.
Action by service representative | Confirm that the optical axis of the tray front detection sensor is not misaligned. Confirm that the product is pushed in by the transport bar of PS-AI.
Related part | Main board, detector board, infeeder tray front detection sensor
Remarks |