- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

#### ■Cutter Cover Error(3051) / Linerless

Error content | The cutter cover of the printer is open.
Detail | Displayed when the cutter cover of the printer is open during printing or blank feeding.
Solution | Set the cutter cover and press the [OK] button.
Action by user | Close the cutter cover.
Action by service representative | Check the cutter cover sensor.
Related part | Main board, Cutter cover sensor
Remarks |