- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

#### ■Cutter of Printer1 Is Abnormal(0769) / Linerless

Error content | The cutter of Printer 1 is abnormal.
Detail | Displayed when the cutter origin sensor does not intercept light during label operation.
Solution | Press the [OK] button. * Cutter unit replacement or cutter origin sensor adjustment is required.
Action by user |
Action by service representative |
Related part |
Remarks | The contents related to the sub error number are as follows: Sub-error "0001" occurs in WM-AI (for DP mode) Sub-error "0002" occurs in WM-AI (during wrapping operation)