- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No label to apply (610)

Error content | No label to apply.
Detail | There was no label when application was attempted. Sub-error meanings are as follows: 0000: Applicator failed in labeled absorption.
Solution | [RETURN] button
Action by user | Clean up the label presence sensor.
Action by service representative | Clean up the label presence sensor.
Related part | ① P-1105 [A100] ② P-1006 [A101] ③ Label presence [B116] ④ Label suction fan [M107]
Remarks |