- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Automatic infeeder is not connected (520)

Error content | The automatic infeeder is not connected.
Detail | The connection of the wire-saving child board is checked when turning on the power or setting up the machine. The P-1105 board for PS-AI was not recognized at this time.
Release method | Follow the on-screen instructions and press the [OK] button.
User’s action | Press the [OK] button. The machine can be used without PS-AI until the power is turned off and on again.
Service action |
Relevant locations | P-1105[A600]
Remarks |