- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

#### ■No label for printer1 (00710-****, 00810-****, 01010-****, 1910-****)

00710-**** | No label for Printer 1 | First upper label printer
00810-**** | No label for Printer 2 | Second upper label printer
01010-**** | No label for Printer 4 | Bottom label printer
01910-**** | No label for Printer 5 | POP label printer

Error content | Printer label finished.
Detail | 0001: Displayed when labels have run out while issuing a label in DP mode. Printer1, Printer2,POP(Printer5) 0002: Displayed when labels have run out while issuing a label with the front cover closed.
Solution | 0001: Press the [OK] button after replacing the label, then performing unloaded feed. 0002: Close the front cover and press the [OK] button after replacing the label, then performing unloaded feed.
Action by user | Same as the solution.
Action by service representative | -Adjust the sensitivity of the label sensory -Check the label sensor
Related part |
Remarks | “Printer No.1” changes depending on error No.