- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Thermal head is worn out for printer 1 (715-0002, 815-0002)

Error content | Thermal head is worn out for printer 1.
Detail | Affected portion is separated by sub-error No. 0002: It has run out in the formatted printing area.
Solution | [EXEC] button, [STOP] button [EXEC]: Head check is performed to the next product. [STOP]；Head check is not performed to the next product.
Action by user |
Action by service representative |
Related part |
Remarks | “Printer No.1” changes depending on error No.