- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film roll driving motor is abnormal (414)

Error content | Film roll driving motor error.
Detail | The roll encoder rotation has not been detected in the film roll driving motor operation. Sub-error meanings are as follows: 0011: The encoder rotation is not detected when the upper film roll is driven. 0021: The encoder rotation is not detected when the lower film roll is driven.
Solution | [RETURN] button
Action by user | Press [RETURN] to release the error.
Action by service representative | Check the following related parts and repair or replace the defective part(s).
Related part | ① P-1105 [A300] ② Upper film roll encoder [B302] ③ Lower film roll encoder [B303]
Remarks |