- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Failed in writing in flash ROM (497)

Error content | Flash ROM write-in error in wrapper program download.
Detail | An error occurred when writing program data received from the wrapper to the flash ROM. Sub-error meanings are as follows: 0001: Flash ROM erasure failure. 0002: Application program flash ROM write-in failure. 0003: Application program sum value flash ROM write-in error. 0004: Message sequence extending to flash ROM write-in is mismatched. 0005: Received a download command even though it is not in boot mode (during application program operation).
Solution | [OK] button
Action by user |
Action by service representative |
Related part | Confirm that all 2, 3 and 4 of DIP switch 1 of P-1105 [A100, A200, A300] are OFF.
Remarks | Re-download