- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Under labeller unit is out (451)

Error content | The under labeller unit is pulled out.
Detail | Stopping in emergency when the under labeller unit sets imperfectly and slips out of the position during the wrapping operation.
Solution | Set the under labeller unit and press [RETURN] button.
Action by user |
Action by service representative |
Related part |
Remarks |
Error content |