- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Motor for film change is abnormal (412)

Error content | The film changing motor is abnormal.
Detail | The operation of the film changing motor has not been completed normally. The sub-error has the following meanings: 0001: The operation is not completed though the operation protection timer has expired. 0011, 12: The film changing outer origin [B309] is light-shielded when the light should not be shielded. 0015/0016: The film changing mechanism moves to the V-shaped position when changing the film. When moving, the film changing inner original position sensor [B304] or the film changing outer original position sensor has been light-shielded. This error occurs when the light is shielded when the light should not be shielded. Check the film changing motor, sensors, and gear gaps. 0020: Neither the film changing inner origin [B304] nor the film changing outer origin [B309] is light-shielded when the insertion operation starts or the changing operation is performed.
Solution | Press the [RETURN] button.
User’s action | Press [RETURN] to release the error.
Service person’s action | Check the following related parts and repair or replace the defective part(s).
Related part | ① P-1105 [A300] ② P-1006 [A301] ③ Stepping motor for changing [M304] ④ film changing inner origin [B304], Film changing outer origin [B309]
Remarks |