- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Temporary blackout on console (407)

Error content | The CPU on the main board (P-1100) of the console has been reset.
Detail | The wrapping board has received the power-on notifying command twice from the main board (P-1100) of the console. For example, this error is displayed without fail after the restart if a problem has arisen with the main board, or if the resetting has been performed without permission. If this error occurs after freezing and resetting, something is wrong with the operation immediately before freezing. For example, when freezing has occurred due to an abnormality of the database, or after various operations have been performed in ADJUST mode (Past instance： The resetting occurred because the main board could not perform normal processing as a result of a foreign language other than English having been input to the product name.) Other than the cases mentioned above, the main board or the switching power supply is suspicious. However, a component of the printer may be short-circuited if it is ineffective in spite of the suspicious board having been replaced.
Solution | When this error occurs, turn on the power source again.
User’s action | Turn on the power source again
Service person’s action |
Related part | ① Main board (1) (P-1100 or P-1163) [A10] ② Switching power supply of the control unit [U10 (Overseas), U11 (Japan)]
Remarks |