- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Abnormal for the position of applicator (617)

Error content | Abnormal for the position of applicator.
Detail | The original point sensor of Y axis was not blocked from light when applicator attempted to start operation.
Solution | [RETURN] button, [PLU] button
Action by user |
Action by service representative |
Related part | ① Y-axis motor [M104] ② Y-axis origin point [B111]
Remarks |