- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

#### ■Thermal head is worn out for printer 1

0715-**** | The thermal head of the printer1 is defective. | Upper label printer 1
0815-**** | The thermal head of the printer2 is defective. | Upper label printer 2
1015-**** | The thermal head of the bottom label printer (printer4) is defective. | Bottom label printer
1915-**** | The thermal head of the printer5 is defective. | POP printer

Error content | The dot (heating element) on the thermal head of the printer is defective.
Detail | The sub-error number tells you where the dot defect is occurring. 0001：The area that does not affect printing is defective. 0002：There is a dot defect in the print format. 0003：The barcode cannot be printed properly. 0004：The part that does not affect printing is defective.
Solution | Touch [Exec] or [Stop] button. [Exec]: Executes the head check for the next product as well. [Stop]: Does not execute the head check for the next product.
Action by user | 0001, 0004: Can be used because it does not affect printing. However, there is a high possibility that other parts will fail due to life expectancy, so contact your dealer. 0002: There is a defect in the print format. It can be used if there is no problem after checking the printed contents of the label. However, there is a high possibility that other parts will fail due to life expectancy, so contact your dealer. 0003: The barcode is cut off. The barcode cannot be read, so contact your dealer.
Action by service representative | 0001, 0004: Can be used because it does not affect printing. However, there is a high possibility that other parts will fail due to life expectancy, so replace the thermal head. 0002：There is a dot defect in the print format. It can be used if there is no problem after checking the printed contents of the label. However, there is a high possibility that other parts will fail due to life expectancy, so replace the thermal head. 0003: The barcode is cut off. The barcode cannot be read, so replace the thermal head.
Related part |
Remarks | “Printer No.1” changes depending on error No.