- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Control board for printer 1 is failed (717-0000, 817-0000, 1917-0000)

Error content | Printer control board error.
Detail | Unable to detect an interrupt signal from the printer control board.
Solution | Restore power.
Action by user |
Action by service representative |
Related part | Printer 1: P-1163 Printer 2: P-1001 POP: P-1131
Remarks | “Printer No.1” changes depending on error number.