- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

■Can Not Communicate With Underlabeller (01001-0000)
■Can Not Communicate With POP Printer (01901-0000)

Error content | Communication error with the printer
Detail | Communication wasn't achieved between the main board and printer board.
Solution | Check the communication line between main board and printer board, then touch [REEXEC]. Touch [STOP] when the error cannot be canceled.
Action by user | Touch [REEXEC].
Action by service representative | 1001-0000：Communication failure between P-1163（P-1100/P-1000) and bottom label printer P-1131 (via USB communication) 1901-0000：Communication failure between P-1163（P-1100/P-1000) and POP label printer P-1131 (via USB communication)
Related part |
Remarks | "Bottom label printer (Printer No.4)" changes depending on error No.