- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Motor for back squeeze plate is abnormal (415)

Error content | Motor for back squeeze plate error.
Detail | Motor for back squeeze plate operation did not finish normally. Sub-error meanings are as follows: 0001: Operation wasn’t completed when the operation protection timer run out. 0003: DCB motor is overloaded. 0004: Feedback pulse from DCB motor has an error (phase interruption). 0011: The origin sensor is not receiving light at the timing with the origin sensor not receiving light.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A100] ② Driving motor for back squeeze plate [M02] ③ Origin point of back squeeze plate [B101]
Remarks |