- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Problem on tray detector (1503)

Error content | The command sent to the applicator and the command contained in the answer is different.
Detail |
Solution | Restore power
Action by user |
Action by service representative | Confirm the RS485 communication line of the main board (P-1100, P-1163, P-1000). Confirm RS485 communication line [A221 XJ-11] and 24 V DC power supply [A221 XJ-9] of the detector board.
Related part | Main board (P-1100, P-1163, P-1000) [A10] Detector board (P-1107) [A221]
Remarks |