- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film removal is completed (492)

Error content | Film removal is completed.
Detail | Film removal operation has been completed. 0000: This error occurs when the film is finished or when the upper film set is required. 0001: This error occurs when the film is finished, when the upper film set is required, or when the film is removed due to some other error. 0002: This error occurs when both the left and right covers need to be opened to check the film after the completion of film removal, such as when the film has overrun.
Solution | 0000: Open the film replacement cover and remove the film. 0001: Open the film replacement cover and remove the film. 0002: Open both the left and right covers to check and remove the film.
Action by user | Same as above
Action by service representative | Check the film passage sensor or film overrun sensor.
Related part |
Remarks |