- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< The loading conveyor motor error (512)

Error content | Error in the loading conveyor motor
Detail | This error occurs when the motor driver of the loading conveyor notifies the alarm. The sub-error has the following meanings: 0001: The operation was not completed even though the operation protection timer expired. 0003: The DCB motor alarm has occurred (overloaded). 0004: The feedback pulse from the DCB motor was abnormal (phase interruption).
Release method | Press the [RETURN] button.
User’s action | Follow the on-screen instructions and press the [RETURN] button.
Service action |
Relevant locations | 1) P-1105[A600] 2) Loading conveyor motor [E601]
Remarks |