- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Insert plate is not set for the lower (479)

Error content | Insert plate is not set for the lower.
Detail | Film exchange cover is closed, but lower film insert open/close is open.
Solution | Press the [RETURN] button after setting the insert plate.
Action by user |
Action by service representative |
Related part | <If the error occurs even after the insert open/close is closed> ① P-1105 [A300] ② Lower film inserts open/close [B305]
Remarks |