- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film is remaining (480－0001)

Error content | Film remains.
Detail | The film detection plate falls down when trying to start film feeding. The sub-error shows the fallen detection plate location using a bit mask. Numbers and the corresponding locations are as follows: 0001: Rear right 0010: Front right 0100: Rear left 1000: Front left (Example) The sub-error becomes 0011 when the remaining film (residue) is detected at the rear right and the front right).
Solution | Remove the film and press the [RETURN] button.
User’s action |
Service person’s action |
Related part | When the error state persists even after the film has been removed ① P-1105 [A200] ② Front right film presence/absence [B209] ③ Front left film presence/absence [B208] ④ Back left film presence/absence [B210] ⑤ Back right film presence/absence [B211] ⑥ The connector of the film street sensor is disconnected.
Remarks |