- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< There is problem on seal heater (473)

Error content | Front outfeed heater error.
Detail | An error occurred in either the front heater or the thermostat monitoring the front heater temperature. Sub-error meanings are as follows: 0000: The heater temperature does not rise while heating (Thermostat value does not change). 0001: Thermostat error (Disconnection or short circuit).
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Outfeed front heater [E70]. ③ Fuse for outfeed heater [F106, F107]. ④ Thermistor for outfeed front heater [R1]. ⑤ SSR for outfeed front heater [K200].
Remarks | The heater is switched OFF when this error occurs.