- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Label is remaining (0351)

Error content | Label is remaining. The label remains on the label applicator (when using hand-pasted labels or bottom labels) Checking the same sensor as in the case of error 0312.
Detail | When the [MENU] key is pressed while the label is not peeled off, an error will be displayed.
Solution | Remove label, [OK] button.
Action by user | Press the [OK] button to finish production.
Action by service representative | Press the [OK] button to finish production. Confirm that there is no actual result remaining error.
Related part | Main board
Remarks |