- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No response from tray detector (1502)

Error content | No response has been received from the detector.
Detail | Communication between the console and the detector has not been performed. The sub-error includes the communication phase number. A communication error immediately after the completion of power-on processing will cause this error.
Solution | Press [STOP] to disconnect the communication with the detector. Operation is possible without label applicator. Press the [REEXEC] button to check the connection with the detector. Release the error after confirming the connection.
User’s action |
Service person’s action | Check the RS485 communication line of the main board (P-100, P-1100, P-1163). Check the RS485 communication line [A221 XJ-11] and the DC 24V power supply [A221 XJ-9] of the detector board.
Related part | Main board (P-100, P-1100, P-1163) [A10] Detector board (P-1107) [A221] The following RS485 communication has not been established: Between P-1107 [A221] (XJ11) and P-1163 [A10] (XJ4)
Remarks |