- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Sensor for the back side of feeder is abnormal (483)

Error content | Sensor for the back side of feeder is abnormal.
Detail | An impossible input combination has occurred in the sensor (Original point, small lift boundary, large lift boundary) detecting the back feeder position. The sub-error screens the input conditions as shown below. 0003: Original point and the small lift boundary sensor are not receiving light. 0005: The small lift boundary sensor and the large lift boundary sensor are not receiving light. 0006: The original point sensor and the large lift boundary sensor are not receiving light. 0007: Three of them are not receiving light.
Solution | [RETURN] button
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Back side of feeder, origin point [B212]. ③ Back side of feeder, position small [B217]. ④ Back side of feeder, position large [B218].
Remarks |