- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

#### ■Label size error for printer1 (00711-0001, 00811-0001, 01011-0001, 011911-0001)

Error content | Label size error for printer 1.
Detail | Error indicates that the format size of producing label in DP mode is different from actual label size.
Solution | Touch [OK] button after removing label by performing the unloaded feed.
Action by user | Touch [OK] button after removing label by performing the unloaded feed.
Action by service representative | Printing was performed, but a label edge was detected at a timing other than the expected timing. -Check the height of the label to be used and the height of the label format. -Adjust the sensitivity of the label sensor -Check the position of the label sensor -Check the advanced feed stop position -Check the back feed amount
Related part |
Remarks | “Printer No.1” changes depending on error No.