- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Film loading instructions (597－0000)

Error content | Film loading instructions.
Detail | Message indicates that the insert plate reached the film set position. Sets the film size or film. [UPPER FILM] sets the upper film size.
Solution | ① Press either the [RETURN] button or the [SET FILM] button. [RETURN]: Returns to the original screen. *Film size returns to the original data. [SET FILM]: Sets the film. ② Open the film exchange cover and close the cover after the film is set.
Action by user |
Action by service representative |
Related part |
Remarks | Sub-error 0000 is displayed when upper film is set.