- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< No connection with applicator (601)

Error content | No connection with applicator.
Detail | ・Communication wasn't achieved between the console and the applicator. ・Communication phase number is in the sub-error. ・Communication errors after power ON result in this error.
Solution | [STOP] => Cut communication with the applicator. Operate without the applicator. [REEXEC] => Check connection with the applicator. The error is cleared if connection is confirmed.
Action by user |
Action by service representative |
Related part |
Remarks | Operation without the applicator is possible after pressing the [STOP] button.