- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Missed to apply POP label (611-2000)

Error content | Failed to apply label on product.
Detail | Sub-error meanings are as follows. 2000: Pasting preparation was not completed when pasting time was run out. 2001: Previous pasting was not completed when pasting timing signal was received. 2002: The tray height message was not received when the pasting timing signal was received.
Solution | Press [RETURN] button.
Action by user |
Action by service representative |
Related part |
Remarks |