- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Product is remaining (0368)

Error content | The front cover was opened when the wrapper stopped and products remained on the lift.
Detail |
Solution | [PLU] button
Action by user | Close the front cover and press the [PLU] key.
Action by service representative | Close the front cover and press the [PLU] key.
Related part | Main board, wrapping machine board
Remarks | * Product is discharged by pressing the [PLU] button. * Added to the total amount.