- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Something is stuck underneath of lift (434)

Error content | An object is caught under the lift.
Detail | Occurs when an overload of lift motor is detected caused by an object caught under the lift. 0000: Operation speed of lift motor is down. 0001: Operation wasn't completed after 5 second since the lift motor has operated.
Solution | [RETURN] button => Restore operation Lift inching => Lift inching operation
Action by user |
Action by service representative |
Related part | ① P-1105 [A200] ② Motor for lift [M06] ③ Lift origin point [B200]
Remarks | Use lift inching to get rid of something caught under the lift.