- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n Label size error for under labeller (1011-0002)

Error content | Label size error for the under labeller.
Detail | Displayed the error that the format size of producing label is different from actual label size when the front cover is closed.
Solution | Remove the under labeller roller or pull the under labeller unit out and perform unloaded feed after removing the label, then press [RETURN] or [PLU] button.
Action by user |
Action by service representative |
Related part |
Remarks | Check the format of label to be printed.