- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

< Infeed conveyor is out (447)

Error content | The infeed conveyor bottom cover was opened during operation.
Detail | Occurs when the infeed conveyor bottom cover is opened while the wrapper is operating
Solution | Press the [RETURN] button after setting the infeed conveyor cover.
Action by user |
Action by service representative |
Related part |
Remarks |