- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

<It cannot differenciate tray (3017)

Error content | It cannot differenciate tray
Detail | This error occurs when the tray cannot be identified while PS-AI is linked.
Solution | Press the [OK] button.
Action by user | When PS-AI is linked, remove the tray and press the [Start] button. For hand-loaded production, re-place the tray.
Action by service representative | When PS-AI is linked, remove the tray and press the [START] button. For hand-loaded production, re-place the tray. On the “CAMERA (ADJUSTMENT)” screen, adjust the brightness and distortion of the detector so that the automatic adjustment functions properly.
Related part | Main board, detector board
Remarks |