- No.100s[System-related Error]
- No.200s[Memory-related Error]
- No.300s, 3000s[Precheck-related Error]
- No.400s, 500s[Wrapper-related Error]
- No.600s[Applicator-related Error]
- No.700s, 800s, 1000s, 1900s[Printer-related Error]
- No.1500s[Detector-related Error]
- No.1600s[Scale-related Error]
- No.1800s,4200s[Dialog Selection-related Error]

n POP Label is remaining on applicator (613-2000)

Error content | Label is remaining on applicator.
Detail | A label remains on the applicator after application.
Solution | Press [RETURN] button after removing the label.
Action by user | Check if the tray height setting matches the actual height.
Action by service representative | Check the value of pasting height adjustment if the pasting control setting of the applicator in adjustment mode is tray height.
Related part |
Remarks |